Type 1 SAP Component: Transition Table

Note: Items marked ( *) are reco mmendations for future inclusion in 188-220A

Transition Input/Event Output/Action

T YPE1SAP-2 DL_Unitdata_Request, no ack

                                                                                                     required

Check to see if destination is receiving. I f so, put UI in the message data structure. If not,

queue the request.

T YPE1SAP-3 DL_Unitdata_Request, ack required Check to see if destination is receiving. I f not, queue the request. Else, put the UI in the

message data str ucture, and set the transmissio n count for that UI to 1.

T YPE1SAP-4 T EST _Request, ack required Check to see if destination is receiving. I f not, queue the request. Else, put the T EST in

the message data structure, and set the transmission count for that T EST  to 1.

T YPE1SAP-5 T EST _Request, no ack required Check to see if destination is receiving. I f so, put T EST in the message data str ucture. If

not, queue the request.

T YPE1SAP-6

T YPE1SAP-9

T YPE1SAP-10

T YPE1SAP-11

T YPE1SAP-12

T YPE1SAP-13

T YPE1SAP-14

                                                                                                     UI Co mmand PDU

                                                                                                     T EST  Response PDU

                                                                                                     T EST  Command PDU P=0

                                                                                                     URR Co mmand PDU

                                                                                                     URR Response PDU

                                                                                                     URNR Co mmand PDU

                                                                                                     URNR Response PDU

Send DL- Unitdata_Ind to Network Layer via Station Co mponent.

Signal initiator of T EST  that response was received. ( *)

Put T EST  Response PDU in message str ucture.

Change sending statio n to NOT  BUSY. Stop busy-state timer (if running).

Mark sender as having sent ack for this PDU. Check if ALL stations which need to ack

have done so. If so, stop the ack timer for this PDU.

Reinforce sending statio n as NOT  BUSY.

Change sending statio n to BUSY.

Start busy-state timer for sending station and mark that station as BUSY.

(Note that receipt of the URNR Response PDU does NOT  constitute ackno wledgement of

corresponding UI Co mmand PDU).

T YPE1SAP-15

T YPE1SAP-16

T YPE1SAP-17

                                                                                                     TP_T IMEOUT  (not N4th trans)

                                                                                                     TP_T IMEOUT  (N4th transmission)

                                                                                                     Busy-state timer timeout

Resub mit the UI which timed out to the message str ucture. Increment the transmissio n

count for that PDU.

Start corresponding busy-state timers. Send DL-State Indication to eventually reach

network layer.

Change statio n which timer -out to NOT  BUSY.

T YPE1SAP-18 Outstanding q ueued request Process next PDU.