Types 1 & 2 Station Component Transition Table:

Common Transitions

Transition Input / Event Output / Action

                     C-1 PL-Unitdata-Ind from physical layer for each deconcatenated DL-PDU

       if valid and dest. address correct

            temporarily place it in deconcatenated DL-PDU queue;

                     C-4 PL-Status- Ind set net-activity variable accordingly;

                     C-5 OP-response-mode- Req set response-mode variable accordingly;

                 C-11 receive: DL-PDU ignore;

                 C-12 receive: DL-Unitdata-Req from Network Layer check QOS information and decide one SAP Component which best serve the

request;

forward the request to appropriate SAP Component chosen;

                 C-13 receive: DL-Unitdata-Ind from Type1 SAP Component forward to Network Layer;

                 C-14 receive: DL-Status- Ind from Type1 SAP Component forward to Network Layer;

                 C-15 receive: DL-Unitdata-Ind from Type2 SAP Component forward to Network Layer;

                 C-16 receive: DL-Status- Ind from Type2 SAP Component forward to Network Layer;

                 C-17 Type2 SAP-message ignore;