Type 2 P-bit Timer: Transition Table

   Transition Input / Event Output / Action

P-TIMER-1 start_P_timer None.

P-TIMER-2 stop_P_timer None.

P-TIMER-3 start_P_timer Allow timer to continue; do not restart.

P-TIMER-4 stop_P_timer None.

P-TIMER-5 P_timer_timeout Send indication that timer has expired