                                                                                 Type 1&4 Station Component Transition Table: Active Phase

Transition Input / Event Output / Action

                               A-1 receive: Type 1 SAP-message buffer message in Station Component message table;

                        A-3-1 receive: DL-PDU from deconcatenated

                                                                                                         DL-PDU queue that requires a coupled

                                                                                                         ack

Stop ACK timer; initiate TP timer processing;

if packet is for SAP component & quiet-mode = OFF & net-activity = CLEAR

then

construct coupled ack and send it in appropriate slot;

if packet is for SAP component, then

         forward to SAP Comp. (with message ID if packet is a coupled ack);

                        A-3-2 receive: DL-PDU from deconcatenated

                                                                                                         DL-PDU queue that does not require a

                                                                                                         coupled ack
if packet is for SAP component, then

         forward to either Type 1 or Type 4 SAP Comp. Accordingly;

                               A-6 Station Component message data

                                                                                                         structure is not empty

                                                                                                         & quiet-mode = OFF

                                                                                                         & net-activity = CLEAR
get highest priority message(s), do FEC, TDC, Scrambling, zero bit stuffing and

concatenate them if feasible to get a Transmission;

send Transmission to Physical Layer;

(save message ID if the message requires coupled ack(s) -- no concatenation)

                        A-7-1 receive: PL-Status- Ind & not expecting

                                                                                                         coupled ack & (transmission-status =

                                                                                                         TRANSMIT COMPLETE, IDLE or

                                                                                                         ABORTED)
set net-activity variable;

process type 4 acks;

                        A-7-2 receive: PL-Status- Ind & expecting

                                                                                                         coupled ack & (transmission-status =

                                                                                                         TRANSMIT COMPLETE, IDLE or

                                                                                                         ABORTED)
start ack timer;

set net-activity variable;

                               A-8 receive: PL-Status- Ind & transmission-

                                                                                                         status = TRANSMIT-IN-PROCESS
set net-activity variable;

                               A-9 receive: ACK-timer-stopped

                           A-10 receive: TP-timer-timeout

                           A-11 receive: Type 4 SAP-message buffer message in Station Component message table;